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ROUTINE VISUAL PLAYGROUND INSPECTION TEMPLATE
In accordance with UK Safety Standard BS EN 1176
Inspector Name: ___________________________ Date: ____ / ____ / 2026
Playground Location: Betchworth Goulborn Green
1. Play Equipment Assets
Inspection Checklist Item Status Notes / Defects Identified
Slide: Check chute for splits/debris, secure handrails, and exposed base footings.
Pass / Fail
Swing: Check chain link wear, top shackle security, and overall frame stability.
Pass / Fail
Rope Ladder: Check for rope fraying, secure knotting, and top/bottom structural anchoring.
Pass / Fail
2. Park Infrastructure & Furniture
Inspection Checklist Item Status Notes / Defects Identified
Public Bench (1 of 2): Check timber slats for splinters, structural rot, and secure ground anchoring.
Pass / Fail
Public Bench (2 of 2): Check timber slats for splinters, structural rot, and secure ground anchoring.
Pass / Fail
Picnic Table: Check for frame wobble, loose assembly bolts, and clean table surface environment.
Pass / Fail
Natural Tree Stumps: Check for wood rot, excessive splitting, splinters, and individual stability.
Pass / Fail
3. General Site Safety & Perimeter
Inspection Checklist Item Status Notes / Defects Identified
Gates & Fences: Check self-closing gate functionality and perimeter fence structural security.
Pass / Fail
Surfacing & Ground: Check rubber impact mats / turf for trip hazards, holes, and open depressions.
Pass / Fail
Cleanliness & Waste: Check for litter, broken glass, dog fouling, and the onsite waste bins are not overflowing.
Pass / Fail
Surrounding Trees: Ensure overhanging branches, brambles or stinging nettles are safely cut back.
Pass / Fail
4. Inspection Sign-Off & Action Plan
Action Required? [ ] Yes [ ] No 
Risk Level Assigned: [ ] Low [ ] Medium [ ] High
Further Actions / Maintenance Orders:
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